{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["Configurator","Config Data"],"not_rendered":{"macros":1,"defined_names":27,"comments":1},"read":"whole","date_system":"1900"}

{"sheet":"Configurator","index":0,"n_rows":13,"n_cols":3,"rows_kept":13,"merged":[[0,0,0,2],[1,0,1,2],[3,0,3,1]]}
["Configured Part Number"]
[{"$f":"CONCATENATE('Config Data'!C2,\"-\",C5,C6,C7,C8,C9,C10,C11,C12,C13)","v":"100X-SH-SF-X-100-120-S-S-R"}]
[]
["Standard Options"]
["Generator","Salt",{"$f":"VLOOKUP(B5,Config_Options,2,0)","v":"S"}]
["Control","Hybrid","H"]
["Flow (lpm)","0-120","-SF"]
["Reagent","NaCl","-X"]
["Pressure (mm H2O)","0-100","-100"]
["Power","120VAC","-120"]
["Chuck","4.5\"","-S"]
["Stroke","Std.","-S"]
["Communication","RS-232","-R"]

{"sheet":"Config Data","index":1,"n_rows":35,"n_cols":4,"rows_kept":35,"hidden":true,"merged":[[3,0,4,0],[6,0,8,0],[10,0,12,0],[14,0,17,0],[19,0,21,0],[23,0,24,0],[26,0,28,0],[30,0,32,0],[34,0,35,0]]}
["Category","Option","Config Codes / Saleable P/N","BOM P/N"]
["100X","100X","100X","100X-CORE"]
[]
["Generator","Salt","S","100X-SALT"]
[null,"Oil","P","100X-OIL"]
[]
["Control","Manual","M","100X-MANUAL"]
[null,"Hybrid","H","100X-HYBRID"]
[null,"Auto","A","100X-AUTO"]
[]
["Reagent","PAO","-P","100X-PAO"]
[null,"DOP","-D","100X-DOP"]
[null,"NaCl","-X","100X-NOOIL"]
[]
["Pressure (mm H2O)","0-25","-025","100X-25MM"]
[null,"0-50","-050","100X-50MM"]
[null,"0-100","-100","100X-100MM"]
[null,"0-250","-250","100X-250MM"]
[]
["Flow (lpm)","0-40","-LF","100X-LOFLOW"]
[null,"0-120","-SF","100X-FLOW"]
[null,"0-180","-HF","100X-HIFLOW"]
[]
["Power","120VAC","-120","100X-120V"]
[null,"240VAC","-240","100X-240V"]
[]
["Chuck","4.5\"","-S","100X-CHUCK"]
[null,"Custom","-C","100X-CUSTOM_CHUCK"]
[null,"AUTO-CTRL","-X","100X-NOCHUCK"]
[]
["Stroke","Std.","-S","100X-STROKE"]
[null,"NO-CHUCK","-X","100X-NOSTROKE"]
[]
[null,"USB","-U","100X-USB"]
["Communication","RS-232","-R","100X-RS232"]